     
     To run the poker program simply type poker and press enter.  please
     read the instructions in the game the first time that you play the
     game.  You can adjust the delays in the program from the command
     line with the /d switch.  So that your synthesizer is not speaking
     at the same time that the wave files are being played.  Such as:
     poker /d 100  100 is the default.
     
     If you have any problems, questions or comments please write or
     call.

     jimkitchen@simcon.net
     http://www.simcon.net/public/jkitchen
     1-440-286-6920
     Chardon Ohio
     
